**Supplementary Materials**

**Biosorption of Oil From Wastewaters By A New Modified Chitosan/Cellulose@Agarose Composite**

**Mustafa A. Ghazalb; Manal G. Mahmoudb\*; Ismail Abeda; Ehsan Abu El-khirb; Mamdouh A. Fahmyb;Laila A. Mohamedb and Alaa E. Alia**

*a Chemistry department, Faculty of Science, Damanhour university, Damanhour, Egypt*

*b Marine Chemistry lab.,National Institute of Oceanography and Fisheries, Cairo, Egypt*

\*Corresponding author e-mail: [manalgom@yahoo.com](mailto:manalgom@yahoo.com)

**Table S1. Equations and parameters of the kinetic models**

|  |  |  |
| --- | --- | --- |
| Kinetic model | Linear equations | Parameters |
| The pseudo – first order | ln(qe–qt) = ln(qe) – k1 t | qe (mg/g) is the amount of adsorbed metal ions at equilibrium  qt (mg/g) is the amount of adsorbed metal ions at time (t)  k1 (min-1) is the pseudo-first order rate constant |
| The pseudo-second order model | t/qt = 1/(k2\*qe2)+(1/qe) t | qt (mg/g) is the amount of adsorbed metal ions at time (t)  k2 (g.mg-1.min-1) is the pseudo-second order rate constant  qe (mg/g) is the amount of adsorbed metal ions at equilibrium |

**Table S2. Equations and parameters of the isotherm models**

|  |  |  |
| --- | --- | --- |
| Isotherm model | Linear equations | Parameters |
| Langmuir isotherm model | Ce /qe = 1/(qm\*KL) + Ce/qm  RL = 1/(1 + KL\*Co) | Ce (mg/L) is the equilibrium concentration of the adsorbate ions  qe (mg/g) is the amount of adsorbed metal ions at equilibrium  qm (mg/g) is the maximum adsorption capacity  KL (L/mg) is Langmuir isotherm constant  RL is the separation factor (0 < RL< 1)  Co (mg/L) is the initial concentration of the adsorbate ions |
| Freundlich isotherm model | log(qt) = log(Kf) + 1/n log(Ce) | qt (mg/g) is the amount of adsorbed metal ions at time (t)  KF (mg/g) is the measure of adsorption capacity (1/n) is the adsorption intensity  Ce (mg/L) is the equilibrium concentration of the adsorbate ions |